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RULES for the Factory Stock races at Mahoning Valley Speedway 2026

The intention of these rules is to help keep costs down.  It is at the discretion of the tech inspector to DQ someone for blatant rule infractions.  Just bring your car and have fun!


BODIES AND FRAMES
1. American made cars 1955 to present with minimum wheel base of 100”.
2. No trucks, sport utility vehicles, station wagons, or front wheel drives.
3. No chopping, channeling or interchanging bodies. 
4. Frame may be repaired at any point from front cross member forward.  Rear frame may be repaired from center of rear, to the rear of the car with 2x3 tubing. 
5. Stock manufactured bodies only.  Internal support structure must remain intact on fenders, quarter panels, hoods and roofs.  Inner body may be gutted only where roll cage will protrude into doors.  Full stock floor panel required.  Trunk floor behind wheel wells may be removed if rear frame is replaced with 2”x 3” box tubing from behind rear axel to rear bumper mounts.  Front wheel wells may be removed but front fenders must remain stock and unaltered.  Front and rear firewall shall remain stock with all flammable material removed and all holes covered with sheet metal.  Stock or aftermarket front and rear bumper covers may be used if for year, make and model.  No spoilers, air dams, skirts or ground effects permitted.  All glass, chrome and taillights must be removed.  Doors must be welded or bolted shut.
6. Cars must have a wire screen or lexan windshield supported inside at center by (3) vertical steel bars minimum 1” x 1/8”, not less than 4 inches apart.  No other windows permitted.  No part of front or rear windshield opening may be obstructed.  No lexan is allowed inside widow openings.
7. All cars must maintain a 5” frame height at all times with driver buckled in seat. 
8. A 2” high non-functioning hood scoop is permitted for air cleaner clearance.  May be fabricated or a stock item.          
                                                         
WEIGHTS AND PERCENTAGES
1. All cars must weight 3200 pounds minimum, after race – with driver.
2. Any add-on weight must be between frame rails, securely bolted to frame, using a minimum of  (2)  3/8” diameter grade A bolts and weight painted white with car number.
3. Maximum of 56% left side weight and no rear weight rule.  



ROLL BARS
1. Minimum  1 ½” X .120” or 1 ¾” X .095” round steel seamless (or DOM) tubing mandatory.
2. All cars are required to have a rear vertical hoop behind and above the drivers’ head, connected to the left and right front roll bar legs by a roof hoop,
3. The front roll bars legs must follow the contour of the windshield post and cowl. 
4. Maximum distance from the windshield to the rear of the roll bar should be no more than 4”.
5. A diagonal bar from the top let to the bottom right must support the vertical rear hoop.
6. A roll bar must connect the left and right of the rear vertical hoop at seat height and across the floor pan at the bottom.
7. An additional bar must be installed at dashboard level, extended from the left front roll bar leg to the right front roll bar leg. 
8. Roll cage must be full perimeter, no offsetting of cages.
9. A minimum of three door bars on the left side and two door bars on the right side must be used.
10. Door bars must be convex in shape and extend into the door panels.
11. Door bars must be attached to each other and the frame with vertical bars.  Minimum of 1/8” X 1” gussets must be welded into all main cage joints and drivers’ door bars.
12. Minimum 1” diameter steel tubing welded directly to the cage must support the drivers’ seat.

RACING SEAT MANDATORY
1. 3” lap belts and 3” shoulder harnesses are mandatory, unless you have a Hans restraint system, then 2 ½”. 
2. Must have a crotch belt.
3. All belts and harnesses must be securely fastened to the cage (harness must be attached below shoulder lever).
4. All belts must be un-frayed and in good appearance.
5. Roll bars in the drivers’ area must be padded.
6. Headrests and drop-down style window nets are mandatory.
7. A radiator hoop may be utilized in the front of the cage with upright supports.
8. Rear cage supports may extend into the rear of the frame.
9. Plating of driver side door bars HIGHLY RECOMMENDED.	   




RUB RAILS/BUMPERS	
1. Rub rails allowed.
2. The top edge of the rub rail is to be no higher than the top of the tire and no lower than the hub center height.
3. Rub rails must be made out of round tubing max 1 ¾" O.D. and will be tight from the inside of rail to the body.
4. One single rub rail per side between wheels.
5. NO other exposed bars allowed.
6. Ends must not be exposed to outside of body skin.
7. Bumpers must be securely mounted.
8. A flat piece of metal must be welded or bolted from outside edge of bumper flush to rear quarter panel and front fender if not using a rubber nose.
9. No sharp edges or cut-off ends.
10. Ends of bumpers must be turned in and sheet metal must be flush to the body to prevent hooking.  
11. Bumpers may be fabricated but must replace stock bumper in stock location.  Fabricated bumpers must be covered with and fit under front and or rear bumper cover.  Tubing in front of the nose piece must be between the frame rails and must mount up against the nose piece.

SUSPENSION
1. Suspension must remain stock and unaltered.
2. Suspension components must be stock to the year, make and model of car being used, with the exception of the sway bar links.  They may be all thread or fastened any other way to top of lower A arm.
3. NO ROD ENDS ALLOWED, MUST BE STOCK IN LOCATION.
4. Urethane rubber or metal suspension bushings may be used.  Must fit into stock control arms without modifications.
5. Stock mount non-adjustable racing shocks permitted.  Only one shock per wheel.
6. Adjustable spring spacers permitted on top of front coil springs, but must accommodate stock mount shocks. 
7. Springs must remain stock type and be mounted in stock location.  Spring rates may be altered.  All cars must maintain a 6” ground clearance at all times, measured from lowest part of frame.
8. Up to 1” factory rubber spring spacer or an adjustable spring spacer allowed on top of rear coil springs.
9. Front strut cars may slot holes to obtain more camber.  Aftermarket camber plates may be used.
10. Stock unaltered sway bars only.  May use threaded rod for sway bar links.
11. All cars must use a retaining hoop at the front and rear of the drive shaft.
12. Drive shaft must be painted white only.
13. No helm joints permitted, magnetic drive shafts only.    
14. Locked rears only.
15. Welded spider or mini-spools permitted.
16. Torque arm cars may mount front of torque arm to frame.  Must use stock mount and remain in stock location.  Welded spider or min-spools permitted.

BRAKES
1. Four-wheel hydraulic brakes in working order are mandatory.
2. No balance bars or adjustable proportioning valves permitted.
3. OEM master cylinders only.
4. No aftermarket master cylinders permitted.
5. OEM calipers and wheel cylinders only.
6. Brake system must be stock for year, make and model.
7. No aluminum brake components.

ENGINE	
1. Engine must match manufacturer of car being used (General Motors in General Motors, Ford in Ford, Mopar in Mopar).
2. All engines will be 358 cubic inch maximum  with a stock stroke and stock bore (+.040 maximum).
3. Maximum compression will be 9.0:1
4. Unaltered OEM cast iron 2 bbl intake manifold only.  No marine or bowtie manifolds permitted.  Edelbrock Performer series manifolds will be allowed.  #2101 for Chevrolets, #2161 for Fords and #2176 for Mopars.
5. Stock unaltered cast iron production cylinder heads only.  No angle plug heads or angle plug Vortec heads.  No bowtie heads. World Products #4266 and #4267 are allowed for Chevrolets and #5303B are allowed for Fords.  Straight plug Vortec heads are allowed. 
6. Stock OEM crankshaft, connecting rods and stock type replacement pistons only.  Eagle connecting rods permitted.  (Part # SIR5700BBLW and SIR5700BPLW for Chevrolet engines.  SIR5956FB and SIR 5956FP for Ford engines.  SIR6123CB for Mopar engines).
7. Stock harmonic balancer or stock type aftermarket replacement balancer allowed.
8. Aftermarket oil pan, valve covers and timing cover allowed.
9. Box stock Holley #4412 carburetor or stock Chevy 2 barrel carburetors only, on maximum one inch thick adapter plate allowed.  Choke components may be removed, must pass all track gauge checks.
10. Solid lifter or hydraulic camshaft permitted.  Hydraulic roller camshaft permitted.  Factory hydraulic roller and retrofit aftermarket hydraulic lifters allowed.  Hydraulic lifters may not be modified what-so-ever.  This includes no spacers or shims.
11. Stock stamped steel rocker arms only.  Stock rocker ratio must be maintained.  No roller or roller tip rocker arms.  No stud girdle.
12. Stock diameter valve springs only.
13. Stock unaltered OEM ignition system only.  Stock replacement aftermarket ignition components may be used.
14. Stock unaltered cast iron rear dump exhaust manifolds only.  No tubular steel factory headers allowed.  If your car comes from a dirt track where headers are allowed.  It will be allowed, but must have 2” exhaust from headers.
15. Engine must be in absolute stock location.  Aftermarket motor mounts allowed (must be exact replacement for stock mounts).  May be solid steel, rubber or polyurethane.  Aftermarket mounts must mount in exact location of stock mounts.
16. GM #602 crate engine will be permitted with box stock Holley #4412 2-barrel carburetor.  Crate motors are subject to tech inspection regardless of seals.  Engine must not be altered in any way.  All parts used must match parts list for GM #602 engine.

ADDITONAL RULES
1. All cars will use a stock unaltered standard or automatic transmission.
2. Standard transmission cars must use a stock steel flywheel, clutch and pressure plate and have a blow proof steel bell housing.
3. Automatic transmission cars must have a stock working torque converter.  Torque converter must be stock diameter and stock stall speed.
4. 2” maximum diameter exhaust and tow Dynomax #24200 track mufflers are mandatory on all cars.
5. No “H” or “X” pipes are permitted.
6. System must be securely fastened, leak free and must exit behind the driver.
7. Mechanical throttle linkage with toe strap and double return springs required.
8. Stock type aftermarket aluminum radiator permitted.  Stock radiator support may be replaced with fabricated unit.  Radiator must mount in stock location.  Transmission coolers must be mounted in engine compartment only.
9. All cars must carry a securely fastened and leak free one-gallon overflow tank.  NO ANTIFREEZE PERMITTED.
10. No rear view mirrors, radios or any other form of driver/crew communication.  Driver MUST monitor one way track scanner and obey and respond to race director’s instructions.  




WHEELS AND TIRES	
1. Steel wheels must be used, 8” wide wheels maximum.  Any offset.
2. Tires – street tires or older Hoosier tires.  Older Hoosier tires 790 or 800 tires.  No new Hoosier tires.  On Hoosier tires there is an oval with a combination of numbers and letters (EX: 1X2Y).  This indicates the year.  If using Hoosier tires you MUST submit a list of tires you are using by providing the number/letter combination of each tire to show you are not using new tires.  If found that you have a 2026 Hoosier tire, you will be disqualified.  Older tires are available at tracks that use them, such as old Evergreen Factory Stock tires, Mahoning and Wall Stadium.  Contact those who race at these tracks and they may give them away.  Street tires that can be used are the Cooper Cobra tires that the Rotten Forgotten run.  Big Diamond Roadrunner tires, Grandview Outlaw tire rules.  Bethel factory stock/street stock tires also allowed.  Cars that run at Bethel may come as is, as per the Bethel rules.  15” passenger tires 205, 215, 225, 235 70/25 street tires must have a tread wear number of no less than 300 and minimum 2/23 of rubber.  Any combination of these tires can be run on your car.
3. No wheel spacers allowed.
4. 1” lug nuts on all four rims are mandatory
5. Any offset wheel permitted.   

FUEL CELLS
1. Encased fuel cell (maximum of 16 gallons) mandatory.  Gasoline only.  Racing gasoline allowed.  Ethanol additives must not exceed 15% of total volume of gasoline.
2. Fuel cell must be centered between rear drive tires mounted as far forward as possible on trunk floor.  If trunk floor is removed behind rear wheels, fuel cell must be mounted to 2” X 3” rear frame section.  Bottom of fuel cell may not be lower than 10” to the ground with driver in seat.  There must be a minimum of a 1” X 1” brace under fuel cell.
3. A minimum 1 ½” bar will be mounted behind fuel cell to ward off puncture.
4. Fuel cell shut off valve must be in plain view, within drivers’ reach.  Shut off valve must be painted fluorescent RED or ORANGE and must be clearly marked “ON” and “OFF”.
5. No electric fuel pumps.
6. No glass or plastic fuel filters.



BATTERY	
1. Battery may be located in the drivers’ compartment.
2. Must be enclosed in a spill-proof container securely fastened to the floor behind driver.
3. All batteries must have a spill or splash cover.
4. A battery shut off switch is mandatory and must be in plain view, painted fluorescent ORANGE or YELLOW and be clearly marked “ON”/”OFF”. 

*****These rules are to keep costs down.  Race cheap and HAVE FUN!*****




