**DOT Rules and CDL Requirements Simplified**

1. According to FMCSA, what is their definition of a commercial vehicle?
	1. Any vehicle used in business to haul equipment, materials, or supplies
	2. Any vehicle requiring the driver to have a CDL
	3. Any vehicle or combination with a GVWR of 10,001 lbs. or greater
	4. Dump trucks, semis, buses, and straight trucks
2. According to FMCSA, a DOT vehicle is required to have what emergency equipment?
	1. A flashing strobe light, blankets, tow straps, and 5 B:C fire extinguisher
	2. Emergency triangles, strobe light, 5 B:C fire extinguisher, and spare fuses
	3. Emergency triangles or fusees, 5 B:C fire extinguisher, and spare fuses
	4. Emergency triangles, 5 B:C fire extinguisher, spare fuses, and CB radio
3. According to FMCSA, a DOT inspection is required when?
	1. Annually
	2. Pre-trip and post-trip
	3. Only when something is wrong
	4. A & B
4. According to FMCSA, regarding drivers and hours of service (HOS) what is the best answer?
	1. Commercial drivers cannot drive more than 8 hours and work more than 12 hours in a day
	2. Commercial drivers must maintain a drivers log regardless of travel distance
	3. Commercial drivers must maintain a drivers log if not taking the 150 air-mile short-haul exemption
	4. Drivers must be able to produce their previous eight consecutive days of record of duty status when asked by authorities
5. According to FMCSA, a DOT recordable accident involves which of the following?
	1. A fatality involving a commercial vehicle
	2. A tow-away of any vehicle involved in the accident involving commercial vehicles
	3. A person requires immediate medical treatment away from the scene of the accident involving a commercial vehicle
	4. All of the above